SAS Luna Microphone/Line Interface

The SAS Luna provides 12 high quality microphone preamps, each with a very wide gain range and individually switchable +48 VDC phantom power. Luna also provides 8 line level fully floating audio outputs. An embedded web server allows configuration and monitoring of inputs and outputs. The Luna pairs well with an SAS Nucleus DSP Engine to provide comprehensive dynamics processing, EQ and AGC.